{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["基础数据模板","车型命名规范","异常类型","产品组与LBTV关联表"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"基础数据模板","index":0,"n_rows":198,"n_cols":19,"rows_kept":198,"flags":["formulas_cached_only"]}
["供应商代码","供应商名称","车型","零件号","零件名称","配置","工位","参数","中值","下公差","上公差","LBTV","奥迪一厂","大众二厂","成都三厂","佛山四厂","青岛五厂","天津六厂","新能源与动力总成"]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8EOL","镜面调节A向角度",-10,-12,-8,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8EOL","镜面调节B向角度",10,8,12,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8EOL","AB向运行电流",55,20,150,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8EOL","AB向卡止电流",80,20,300,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8EOL","C向角度",10,8,12,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8EOL","D向角度",-10,-12,-8,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8EOL","CD向运行电流",55,20,150,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8EOL","CD向卡止电流",80,20,300,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8EOL","AB记忆电阻",4200,3200,5200,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8EOL","CD记忆电阻",4200,3200,5200,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8EOL","电动折叠运行电流",200,20,400,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8EOL","电动折叠卡止电流",1200,20,3000,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8EOL","转向灯电流",90,80,100,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8EOL","电加热电流",2000,1500,2500,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8EOL","SWA电流",50,30,70,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8EOL","LOGO灯电流",147,132,162,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8EOL","镜面拔脱力",130,90,170,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8注塑","1区成型温度",270,260,280,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8注塑","2区成型温度",265,255,275,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8注塑","3区成型温度",260,250,270,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8注塑","4区成型温度",250,240,260,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8注塑","5区成型温度",240,230,250,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8注塑","1段射出压力",95,85,105,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8注塑","2段射出压力",115,105,125,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8注塑","3段射出压力",65,55,75,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8注塑","4段射出压力",58,48,68,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8注塑","1段注射速度",25,15,35,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8注塑","2段注射速度",85,75,95,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8注塑","3段注射速度",45,35,55,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8注塑","4段注射速度",30,20,40,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8注塑","1段保压压力",60,50,70,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8注塑","2段保压压力",20,10,30,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8注塑","1段保压时间",13,10,16,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8注塑","2段保压时间",2,1,3,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8注塑","1段合模压力",35,25,45,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8注塑","2段合模压力",35,25,45,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8注塑","3段合模压力",40,30,50,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8注塑","低压模保",50,40,60,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8注塑","高压模保",150,140,160,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8注塑","烘料温度",90,80,100,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8折叠","折叠正向扭矩",15,10,20,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8折叠","折叠负向扭矩",15,10,20,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8实验室","曲率半径",1230,1200,1260,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8实验室","色差",0.9,1.4,0.1,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8实验室","底漆膜厚",25,2,50,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8实验室","色漆膜厚",25,10,35,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8实验室","清漆膜厚",30,20,40,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8实验室","镜片反射率",40,40,9000,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8实验室","装饰罩重量 L",140,135,145,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8实验室","装饰罩重量 R",142,137,147,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8实验室","前处理PH值",1.7,1,2.5,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8实验室","前处理电导率",37,0,75,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8实验室","弹簧线径",4.25,4.215,4.285,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8实验室","弹簧压缩力",620,560,680,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8实验室","附着力",0,1,0,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8涂装","底漆喷房温度",25,22,28,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8涂装","底漆喷房湿度",65,55,75,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8涂装","色漆喷房温度",25,22,28,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8涂装","色漆喷房湿度",65,55,75,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8涂装","清漆喷房温度",25,22,28,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8涂装","清漆喷房湿度",65,55,75,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8涂装","清漆烘箱温度",90,83,97,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","GolfA8","5HG857501|5HG857502","左/右后视镜总成","无","GolfA8涂装","表面张力",40,30,300,"马健成|任杰",{"$nulls":3},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3EOL","镜面调节A向角度",-9,-10.5,-8.5,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3EOL","镜面调节B向角度",9,8.5,10,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3EOL","AB向运行电流",55,20,150,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3EOL","AB向卡止电流",80,20,300,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3EOL","C向角度",9,8.5,13.5,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3EOL","D向角度",-9,-10,-8.5,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3EOL","CD向运行电流",55,20,150,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3EOL","CD向卡止电流",80,20,300,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3EOL","AB记忆电阻",4200,3200,5200,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3EOL","CD记忆电阻",4200,3200,5200,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3EOL","电动折叠运行电流",400,20,850,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3EOL","电动折叠卡止电流",1600,1275,3000,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3EOL","转向灯电流",120,110,300,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3EOL","电加热电流",1800,1700,2400,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3EOL","SWA电流",76,56,96,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3EOL","摄像头电流",65,40,90,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3EOL","EC电流",100,40,400,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3EOL","镜面拔脱力",100,50,150,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3注塑","1区成型温度",265,255,275,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3注塑","2区成型温度",260,250,270,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3注塑","3区成型温度",245,235,255,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3注塑","4区成型温度",240,230,250,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3注塑","5区成型温度",230,220,240,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3注塑","1段射出压力",95,85,105,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3注塑","2段射出压力",105,95,115,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3注塑","3段射出压力",95,85,105,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3注塑","4段射出压力",90,80,100,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3注塑","1段注射速度",20,10,30,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3注塑","2段注射速度",70,60,80,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3注塑","3段注射速度",60,50,70,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3注塑","4段注射速度",50,40,60,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3注塑","1段保压压力",75,65,85,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3注塑","2段保压压力",35,25,45,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3注塑","1段保压时间",6,4,8,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3注塑","2段保压时间",2,1,3,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3注塑","1段合模压力",30,20,40,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3注塑","2段合模压力",20,10,30,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3注塑","3段合模压力",25,15,35,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3注塑","低压模保",30,20,40,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3注塑","高压模保",150,140,160,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3注塑","烘料温度",105,100,110,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3折叠","折叠正向扭矩",14.5,10,19,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3折叠","折叠负向扭矩",14.5,10,19,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3实验室","曲率半径",1230,1200,1260,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3实验室","色差",0.7,1.4,0.1,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3实验室","底漆膜厚",25,2,50,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3实验室","色漆膜厚",25,10,35,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3实验室","清漆膜厚",30,20,40,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3实验室","镜片反射率",40,40,9000,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3实验室","装饰罩重量 L",127,122,132,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3实验室","装饰罩重量 R",136,131,141,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3实验室","前处理PH值",1.7,1,2.5,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3实验室","前处理电导率",37,0,75,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3实验室","弹簧线径",4.25,4.215,4.285,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3实验室","弹簧压缩力",780,710,850,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3实验室","附着力",0,1,0,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3涂装","底漆喷房温度",25,22,28,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3涂装","底漆喷房湿度",65,55,75,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3涂装","色漆喷房温度",25,22,28,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3涂装","色漆喷房湿度",65,55,75,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3涂装","清漆喷房温度",25,22,28,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3涂装","清漆喷房湿度",65,55,75,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3涂装","清漆烘箱温度",90,83,97,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","AudiA3Spb.|AudiA3Lim.","8YG858499|8YG858500","左/右后视镜总成","无","AudiA3涂装","表面张力",40,30,300,"李晓东|任杰",{"$nulls":4},1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","TavendorEOL","A向运行电流",55,40,100,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","TavendorEOL","A向运行角度",9,8,10,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","TavendorEOL","A向卡止电流",80,50,500,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","TavendorEOL","A向记忆电压",1.1,0.3,1.7,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","TavendorEOL","B向运行电流",55,40,100,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","TavendorEOL","B向运行角度",9,8,10,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","TavendorEOL","B向卡止电流",80,50,500,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","TavendorEOL","B向记忆电压",4,3,5,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","TavendorEOL","C向运行电流",55,40,100,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","TavendorEOL","C向运行角度",9,8,10,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","TavendorEOL","C向卡止电流",80,50,500,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","TavendorEOL","C向记忆电压",5,3,5,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","TavendorEOL","D向运行电流",55,40,100,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","TavendorEOL","D向运行角度",9,8,10,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","TavendorEOL","D向卡止电流",80,50,500,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","TavendorEOL","D向记忆电压",1,0.3,1.7,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","TavendorEOL","折叠运行电流",550,100,1000,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","TavendorEOL","折叠卡止电流",1500,500,2400,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","TavendorEOL","转向灯电流",70,30,163,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","TavendorEOL","电加热电流",3000,1000,3700,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","TavendorEOL","SWA电流",30,20,45,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","TavendorEOL","摄像头电流",70,57,83,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","TavendorEOL","EC电流",200,100,400,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","TavendorEOL","镜面拔脱力",100,90,150,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor注塑","1区成型温度",270,260,280,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor注塑","2区成型温度",265,255,275,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor注塑","3区成型温度",260,250,270,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor注塑","4区成型温度",250,240,260,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor注塑","5区成型温度",240,230,250,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor注塑","1段射出压力",90,80,100,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor注塑","2段射出压力",95,85,105,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor注塑","3段射出压力",85,75,95,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor注塑","4段射出压力",75,65,85,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor注塑","1段注射速度",45,35,55,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor注塑","2段注射速度",60,50,70,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor注塑","3段注射速度",55,45,65,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor注塑","4段注射速度",45,35,55,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor注塑","1段保压压力",85,75,95,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor注塑","2段保压压力",40,30,50,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor注塑","1段保压时间",10,7,13,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor注塑","2段保压时间",2,1,3,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor注塑","1段合模压力",35,25,45,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor注塑","2段合模压力",35,25,45,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor注塑","3段合模压力",40,30,50,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor注塑","低压模保",50,40,60,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor注塑","高压模保",150,140,160,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor注塑","烘料温度",90,80,100,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor折叠","折叠正向扭矩",14,10,18,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor折叠","折叠负向扭矩",14,10,18,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor实验室","曲率半径",1230,1200,1260,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor实验室","色差",0.9,1.4,0.1,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor实验室","底漆膜厚",25,2,50,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor实验室","色漆膜厚",25,10,35,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor实验室","清漆膜厚",30,20,40,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor实验室","镜片反射率",50,40,9000,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor实验室","装饰罩重量 L",127,122,132,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor实验室","装饰罩重量 R",136,131,141,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor实验室","前处理PH值",1.7,1,2.5,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor实验室","前处理电导率",37,1,75,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor实验室","弹簧线径",4.25,4.215,4.285,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor实验室","弹簧压缩力",780,710,850,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor实验室","附着力",0.5,1,0,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor涂装","底漆喷房温度",25,22,28,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor涂装","底漆喷房湿度",65,55,75,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor涂装","色漆喷房温度",25,22,28,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor涂装","色漆喷房湿度",65,55,75,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor涂装","清漆喷房温度",25,22,28,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor涂装","清漆喷房湿度",65,55,75,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor涂装","清漆烘箱温度",90,83,97,"常丹|任杰",null,1]
["5AD","上海干巷车镜实业有限公司","Tavendor","30C857501|30C857502","左/右后视镜总成","无","Tavendor涂装","表面张力",40,30,300,"常丹|任杰",null,1]

{"sheet":"车型命名规范","index":1,"n_rows":35,"n_cols":3,"rows_kept":35,"merged":[[1,1,4,1],[5,1,10,1],[11,1,14,1],[15,1,20,1],[21,1,23,1],[24,1,27,1],[28,1,31,1]],"flags":["formulas_cached_only"]}
["序号","质保部","车型标准名称"]
[1,"奥迪质保部","AudiA6L"]
[2,null,"AudiA4L"]
[3,null,"AudiQ5L"]
[4,null,"AudiQ5LDerivat"]
[5,"大众质保部","Magotan"]
[6,null,"CCFB"]
[7,null,"CCSHB"]
[8,null,"Talagon"]
[9,null,"Tavendor"]
[10,null,"Tacqua"]
[11,"成都质保部","SagitarPA"]
[12,null,"JettaVA3"]
[13,null,"JettaVS5"]
[14,null,"JettaVS7"]
[15,"佛山质保部","GolfA8"]
[16,null,"T-ROCPA"]
[17,null,"AudiQ2L"]
[18,null,"ID.4CROZZ"]
[19,null,"ID.6CROZZ"]
[20,null,"AudiQ4e-tron"]
[21,"青岛质保部","BoraMQBPA"]
[22,null,"AudiA3Spb."]
[23,null,"AudiA3Lim."]
[24,"天津质保部","TayronPA"]
[25,null,"TayronXPA"]
[26,null,"AudiQ3"]
[27,null,"AudiQ3Spb."]
[28,"新能源与动力总成"]
[29]
[30]
[31]
[]
[]
["规则：将质量周报系统中车型名称中空格去掉，有其他车型或变化请联系丁善刚"]

{"sheet":"异常类型","index":2,"n_rows":15,"n_cols":2,"rows_kept":15,"flags":["formulas_cached_only"]}
[]
[null,"产品类-尺寸"]
[null,"产品类-材料"]
[null,"产品类-外观"]
[null,"产品类-性能"]
[null,"过程类-人员"]
[null,"过程类-机器"]
[null,"过程类-物料"]
[null,"过程类-方法"]
[null,"过程类-环境"]
[null,"过程类-测量"]
[null,"设备类-硬件调试"]
[null,"设备类-软件设定"]
[null,"测试类-系统接入准备"]
[null,"其他类非质量报警"]

{"sheet":"产品组与LBTV关联表","index":3,"n_rows":48,"n_cols":3,"rows_kept":48,"flags":["formulas_cached_only"]}
[null,"产品组","L-BTV"]
[1,"螺旋弹簧","李书博"]
[2,"前中扶手","张恒伟"]
[3,"外后视镜","任杰"]
[4,"顶棚","李峰"]
[5,"门把手","李晓东"]
[6,"仪表板骨架","李英强"]
[7,"门护板","姜薇"]
[8,"减震器","殷孟游"]
[9,"前照灯","赵晴华"]
[10,"方向盘","张兆春"]
[11,"尾灯","贾琼雪"]
[12,"制动盘","周璟琤"]
[13,"燃油箱","张永辉"]
[14,"天窗","孙金录"]
[15,"转向柱","高升光"]
[16,"后盖锁","陈宏杰"]
[17,"雨刮","孟庆宇"]
[18,"手套箱","袁泉"]
[19,"蓄电池","张国鑫"]
[20,"仪表板","吴玉杰"]
[21,"车门装饰条","金江"]
[22,"燃油泵","张永辉"]
[23,"前座椅骨架","邸玥昕"]
[24,"车门外密封条","郑静"]
[25,"头枕","张慎之"]
[26,"压缩机","刘欣"]
[27,"方向盘开关","陈曦"]
[28,"冷凝器","阳鹏"]
[29,"转向柱开关","董怀力"]
[30,"出风口","熊建秋"]
[31,"散热器","胡建国"]
[32,"玻璃升降器","熊昕"]
[33,"遮阳板","邓律华"]
[34,"多功能摄像头","尹星"]
[35,"倒车影像","王建吉"]
[36,"屏幕","刘晓"]
[37,"后门窗导轨","吕晓芳"]
[38,"扬声器","杨爱均"]
[39,"座椅安全带","刘景景"]
[40,"前后保险杠","冯振川"]
[41,"座椅总成","孙金录"]
[42,"车门装饰条","杨欢"]
[43,"车轮装配总成","赵礼东"]
[44,"天窗排水管","崔楠"]
[45,"铝车轮","高升光"]
[46,"动力总成电子执行器","杜君"]
[47,"MEB继电器","张霄宇"]